BIOS Hauptmenü

AMIBIOS SIMPLE SETUP - UTILITY ‑ VERSION 1.21.11
(C)2000 American Megatrends, Inc. All Rights Reserved

Standard CMOS Setup	Features Setup

Advanced Setup	CPU PnP Setup

Power Management Setup	Hardware Monitor

PCI / Plug and Play Setup	Change Password

Load Optimal Settings	Exit

Load Best Performance Settings

ESC: Quit   E Select Item   (Shift)F2: Change Color      F5: Old Values
F6: Optimal values      F7: Best performance values      F10: Save&Exit

Standart CMOS Setup spezifische Einstellung

Standard CMOS setup for changing time, date, hard disk type, etc.

AMIBIOS SETUP ‑ STANDARD CMOS SETUP
(C)2000 American Megatrends, Inc. All Rights Reserved

Date (mm/dd/yyyy): Sat Jan 31,2004

Time (hh/mm/ss)	23:07:27
		LBA Blk	PIO 	32Bit

	Type		Size	Cyln 	Head WPcom Sec Mode Mode Mode Mode

Pri	Master	:User	80.OGB	38297 16	0	255 On	On	4	On
Pri	Slave	:Not Installed
Sec	Master	:DVD‑ROM						4	On
Sec	Slave	:CDROM						4	On

Floppy Drive A: 1.44 MB 3%
Floppy Drive B: Not Installed

Month:	Jan ‑ Dec	ESC	: Exit
Day:	01 ‑ 31	E	: Select Item
Year: 1980 ‑ 2099	 PU/PD/+/‑ : Modify
		 (Shift)F2 : Color
		 F3 : Detect All HDD

Standart CMOS Setup allgemingültige Einstellung

AMIBIOS SETUP ‑ STANDARD CMOS SETUP
(C)2000 American Megatrends, Inc. All Rights Reserved

Date (mm/dd/yyyy): Sat Jan 31,2004

Time (hh/mm/ss)	23.05:32
		LBA Blk	PIO	32Bit

	Type		Size	Cyln	Head WPcom Sec Mode Mode Mode Mode
	Pri Master :Auto					On
Pri Slave	:Auto					On
	Sec Master :Auto					On
Sec Slave	:Auto					On

Floppy Drive A: 1.44 MB 3%
Floppy Drive B: Not Installed

Month:	Jan ‑ Dec	ESC	: Exit
Day:	01 ‑ 31	E	: Select Item
Year: 1980 ‑ 2099	 PU/PD/+/‑ : Modify
		 (Shift)F2 : Color
		 F3 : Detect All HDD

Advanced Setup

	AMIBIOS SETUP ‑ ADVANCED SETUP
(C)2000 American Megatrends, Inc. All Rights Reserved

Quick Boot	Enabled	CLK GEN Spread Spectrum	Disabled
lst Boot Device	IDE‑0	DOS Flat Mode	Disabled
2nd Boot Device	Disabled	Dram Driver Slew Rating 	Normal
3rd Boot Device	Disabled	S2K I/0 Compensation	Disabled
Try Other Boot Devices	No
S.M.A.R.T. for Hard Disks    Enabled
BootUp Num‑Lock	On
Floppy Drive Swap	Disabled
Floppy Drive Seek	Disabled
Password Check	Setup
Boot To OS/2 > 64MB	No
Ll Cache	Enabled
L2 Cache	Enabled
System BIOS Cacheable	Enabled
Graphic Win Size	64M
DRAM Timing Configuration	Safe 	ESC	: Quit	E Select Item
SDR/DDR CAS Latency	3T	Fl	: Help	PU/PD/+/‑ : Modify
SDR/DDR RAS Active Time	7T	 F5	: Old Values (Shift)F2 : Color
SDR/DDR RAS Precharge Time   4T	 F6	: Load Optimal Values
Auto Detect DIMM/PCI Clk	Enabled	 F7	: Load Best Performance Values

Power Management Setup

	AMIBIOS SETUP ‑ POWER MANAGEMENT SETUP
(C)2000 American Megatrends, Inc. All Rights Reserved

ACPI Aware O/S	Yes
Power Management	Enabled
Suspend Time Out	Disabled
Hard Disk Time Out	Disabled
PowerOn by LAN/Ring	Disabled
RTC Alarm Power On	Disabled
RTC Alarm Date	Every Day
RTC Alarm Hour	12
RTC Alarm Minute	30
RTC Alarm Second	00
Keyboard PowerOn Function Disabled

ESC : Quit        E Select Item
Fl  : Help PU/PD/+/‑ : Modify
F5  : Old  Values (Shift)F2 : Color
F6  : Load Optimal Values
F7  : Load Best Performance Values

PCI / Plug and Play Setup

	AMIBIOS SETUP ‑ PCI / PLUG AND PLAY SETUP
(C)2000 American Megatrends, Inc. All Rights Reserved

Plug and Play Aware O/S	Yes
AGP 4X Control	Enable
Primary Graphics Adapter	AGP
Allocate IRQ to PCI VGA 	Yes
PCI IDE BusMaster	Enabled

ESC : Quit  E Select Item
Fl  : Help    PU/PD/+/‑ : Modify
F5  : Old Values (Shift)F2 : Color
F6  : Load Optimal Values
F7  : Load Best Performance Values

Features Setup

	AMIBIOS SETUP ‑ FEATURES SETUP
(C)2000 American Megatrends, Inc. All Rights Reserved

OnBoard FDC	Enabled
0nBoard Serial PortA	3F8h/C0M1
OnBoard Serial PortB	2F8h/COM2
	Serial Port2 Mode	Normal
OnBoard Parallel Port	378h
	Parallel Port Mode	EPP+ECP
	Parallel Port IRQ	7
	Parallel Port DMA	3
0nBoard Game Port	201h
0nBoard MIDI Port	300h
	MIDI Port IRQ	10
Onboard PCI IDE	Both
0nBoard AC'97 Sound	Enabled
OnBoard AC´97 MODEM	Disabled
OnBoard LAN	Enabled
USB Function Support	Enabled	
USB Function for DOS	Disabled	
ThumbDrive Support for DOSDisabled	

                                              ESC : Quit      E Select Item
                                              Fl : Help PU/PD/+/‑ : Modify
                                              F5 : Old Values (Shift)F2 : Color
	F6 : Load Optimal Values
	F7 : Load Best Performance Values

CPU PnP Setup

	AMIBIOS SETUP ‑ CPU PnP SETUP
(C)2000 American Megatrends, Inc. All Rights Reserved

CPU BRAND	AMD K7
CPU Type	Athlon XP
CPU Speed	133/133MHz
CPU Core Voltage	1.728 V
CPU Frequency	133MHz
DRAM Frequency	133MHz
		 ESC : Quit	E Select Item
		 F1 : Help	PU/PD/+/‑ : Modify
                                             F5: Old Values (Shift)F2 : Color
                                             F6: Load Optimal Values
                                             F7: Load Best Performance Values